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SPECIFICATION 204
ENVIRONMENTAL MANAGEMENT

	[bookmark: _Toc136503052][bookmark: _Toc214962339]GENERAL
	

	[bookmark: _Toc136503053][bookmark: _Toc214962340]204.01	Scope
	

	This specification outlines the minimum requirements for establishing, implementing and managing an Environmental Management Plan (EMP) for the work under the Contract.
	

	The Contractor must establish, implement and manage a contract-specific EMP that addresses the Principal’s minimum environmental and heritage requirements through the application of Operational Controls.
	

	This specification applies to all work under the Contract, including activities that may be undertaken in connection with the Contract that are not located on the Site.
	

	This specification is based on AS/NZS ISO 14001.
	

	[bookmark: _Toc136503054][bookmark: _Toc214962341]204.02	References
	

	1. Australian Standards, Main Roads Western Australia Test Methods, Main Roads Western Australia Standards and Main Roads Western Australia Specifications are referred to in abbreviated form (e.g. AS 1234, MRS 67-08-43 or WA 123).  For convenience, the full titles are given below:
	

		Acts and Regulations
	

		Environment Protection and Biodiversity Conservation Act 1999
	Environmental Protection Act 1986
	Aboriginal Heritage Act 1972
	Biodiversity Conservation Act 2016
	Country Areas Water Supply Act 1947
	Contaminated Sites Act 2003
	Heritage Act 2018
	Rights in Water and Irrigation Act 1914
	Swan and Canning Rivers Management Act 2006
	

		Australian / New Zealand International Standards
	

		AS/NZS ISO 14001	Environmental Management Systems, specification with guidance for use
	AS/NZS ISO 31000	Risk Management
	

		MAIN ROADS Specifications
	

		Specification 100	GENERAL REQUIREMENTS
	Specification 201	QUALITY MANAGEMENT
	Specification 203	HEALTH AND SAFETY MANAGEMENT
	Specification 301	VEGETATION CLEARING AND DEMOLITION
	Specification 302	EARTHWORKS
	Specification 303	MATERIAL AND WATER SOURCES 
	Specification 304	LANDSCAPING AND REVEGETATION / REHABILITATION OF DISTURBED AREAS / REVEGETATION
	

	[bookmark: _Toc214962342]204.03	Definitions
	

	1. The meaning of terms and definitions in this specification are as defined in AS/NZS ISO 14001.  The following particular definitions also apply:
	

	Designated Area
	means an area that is not a vegetated area and has been approved by the Superintendent.
	

	Environmental and Heritage Aspect
	means an element of an activity, product, or service that can interact with the environment or heritage.  An Environmental or Heritage Aspect can cause an Environmental or Heritage Impact.
	

	Environmental and Heritage Impact
	means any change to the environment or heritage, whether adverse or beneficial, wholly or partially resulting from a Contract’s environmental or heritage aspects.
	

	Environmental Incident
	means an unplanned event resulting in or having the potential for environmental or heritage impact or other loss.
	

	Environmental Management Plan (EMP)
	means the approved management document that contains the Contractor’s identified Environmental and Heritage Aspects, Environmental and Heritage Impacts, the risks associated with the identified aspects and impacts, and the control measures that will be put in place to manage the impacts.  Refer to Annexure 204A.
	

	Environmental Management Representative (EMR)
	is the person appointed by the Contractor’s Representative with defined authority and responsibility to implement the environmental management plan.
	

	Limits of Activity
	means the area of work under the Contract. The Limits of Activity must contain the Limits of Vegetation Clearing.
	

	Limits of Vegetation Clearing 
	as per the definition in Specification 301 VEGETATION CLEARING AND DEMOLITION.
	

	Maintenance Environmental Management Plan (MEMP) Template
	means the template supplied by the Principal that details the minimum environmental and heritage requirements that the Contractor is to address.  The Contractor must use the MEMP template to develop their own MEMP for works under the Contract.  The MEMP template is provided in Annexure 204A.
	

	Operational Controls
	means specific operations for controlling and managing the activities, processes, products, and services associated with the Environmental and Heritage Aspects.
	

	Principal Environmental Work Requirements (PEWR)
	means a document supplied by the Principal that details the minimum environmental and heritage requirements for low risk and low complexity works.  Where a PEWR is provided by the Principal, the Contractor is not required to develop an EMP, but instead must comply with, and sign-on to, the controls listed in the PEWR.
	

	Regulator
	means a government agency that is responsible for the administration of legislation (e.g. Department of Water and Environmental Regulation).
	

	Risks and Opportunities
	means potential adverse effects (threats) and potential beneficial effects (opportunities) in relation to environment and heritage.
	

	Short Term Worker
	is a Worker who is on the Site generally less than one (1) work shift to perform work, deliver goods or conduct visual observation.
	

	Site
	as defined in the Contract plus any other location where work under the Contract is being undertaken.
	

	Visitor
	is a person visiting the Site for a purpose associated with the work under the Contract who is not conducting any work.
	

	Worker
	has the same meaning as Part 1 Division 3 (7) of the WHS Act (WA) 2020, but excludes the Principal’s Personnel.
	

	[bookmark: _Toc214962343]204.04 – 204.05	NOT USED
	

	[bookmark: _Toc214962344]ENVIRONMENTAL POLICY
	

	[bookmark: _Toc214962345]204.06	Main Roads Environmental Policy
	

	1. Main Roads Environmental Policy outlines Main Roads commitment to environmental management principles and objectives that provide the overall intentions and direction of the organisation.  All people working on behalf of Main Roads must be aware of the Policy, its purpose and their role in achieving the commitments, including how their work can affect Main Roads ability to fulfil its compliance obligations.
	Environmental Policy

	1. Main Roads Environmental Policy is located under Environment on the Main Roads website at environmental-policy.pdf (mainroads.wa.gov.au).
	

	1. The Contractor must prominently display a copy of Main Roads Environmental Policy on the Site Office Notice Board for the duration of the work under the Contract and include it in information provided to persons at the Contract induction.  The Policy must also be available to each subcontractor.
	Communication

	1. Main Roads Environmental Policy must be communicated to all on site personnel.
	

	[bookmark: _Toc214962346]204.07 – 204.15	NOT USED
	

	[bookmark: _Toc214962347]PLANNING
	

	[bookmark: _Toc214962348]204.16	Legal and Other Compliance Requirements
	

	1. The Contractor must identify and have access on site to all relevant legal and other requirements that are applicable to the Environmental and Heritage Aspects of the activities associated with work under the Contract.
	Environmental Compliance Obligations

	1. Planning undertaken by the Principal will be detailed in the EMP.  Compliance obligations that have been delegated to the Contractor are detailed in Annexure 204B.
	

	1. The Contractor must present the Limits of Activity in a figure in the EMP.  A figure(s) will show the area(s) to which the EMP applies for work under the Contract. 
	EMP Coverage

	1. Annexure 204B details the requirements that contain HOLD POINTS and WITNESS POINTS.  The Contractor must outline how these will be managed in the EMP.
	Hold Points and Witness Points

	1. The Contractor must determine how relevant environmental and heritage legal and other requirements apply to the work under the Contract.
	Legal and Other Requirements

	1. Application of the Contract requirements, Standards and Codes of Practice in no way relieves the Contractor from undertaking any activity, function, process or procedure necessary to meet the legislation and regulation listed in Clause 204.02 References or any other relevant legislation or standards.
	

	[bookmark: _Toc214962349]204.17	Risks and Opportunities
	

	1. During the preparation of the EMP, the Contractor must conduct an assessment of Risks and Opportunities of work under the Contract to identify those activities with significant potential to impact Environment and Heritage Aspects.
	

	1. The identified Risks and Opportunities must be detailed in the EMP.
	Documenting Risks and Opportunities

	1. The Contractor must develop Operational Controls to manage the identified Risks and Opportunities and detail these in the EMP.
	

	[bookmark: _Toc214962350]204.18	Environmental Management Plan 
	

	1. The Contractor must populate the delegated sections in the EMP template in Annexure 204A.
	EMP Template

	1. Any person engaged to undertake any work under the Contract, including subcontractors, must be required to comply with the approved EMP while undertaking the work.
	

	1. If not submitted and explicitly approved in writing during the Tendering process, the Contractor must submit a suitably documented EMP to the Superintendent for approval no less than 14 days prior to the intended start date of physical work under the Contract.
	

	1. No physical work under the Contract shall be undertaken by the Contractor until the EMP is approved by the Superintendent.
	HOLD POINT

	1. [bookmark: _Hlk116554299]For Works under a PEWR, all on site contractors, including subcontractors, must sign the PEWR prior to commencing the works.  By signing the PEWR personnel are demonstrating they have understood the requirements of the PEWR, commit to ensuring their Operational Controls address the requirements in the PEWR, and they will implement their Operational Controls for the duration of the work under the Contract.
	PEWR

	[bookmark: _Toc214962351]204.19 – 204.20	NOT USED
	

	[bookmark: _Toc214962352]IMPLEMENTATION
	

	[bookmark: _Toc214962353]204.21	Roles and Responsibilities
	

	1. The Contractor must clearly define, document and communicate the environmental responsibilities and accountabilities of all Contract management personnel, employees and subcontractors.
	Responsibilities

	1. The Contractor is directly responsible for environmental management and control of all activities relating to the execution of the work under the Contract including work under the Contract undertaken by subcontractors.
	Contractor

	1. The EMP must detail procedures and processes that the Contractor will implement to ensure subcontractors always comply with the requirements of the approved EMP.
	Subcontractors

	1. The Contractor must appoint a competent Environmental Management Representative (EMR) for the duration of the work under the Contract and document them in the EMP.  Prior to commencement of site work under the Contract, the EMR must have completed the Principal’s EMR eLearning module.  The EMR must generally be in attendance on the site at all times when activities relating to the execution of the work under the Contract are taking place, and have the necessary authority and resources to meet their responsibilities to implement the EMP. 
	EMR

	1. The EMR has the authority to delegate their responsibilities to an on-site person for short periods and only for low-risk activities.
	EMR Delegate

	1. The EMR must be responsible for:
(a) taking accountability for the effectiveness of the EMP;
(b) ensuring the integration of the EMP into the planning of project delivery;
(c) ensuring resources are available for the implementation of the EMP;
(d) communicating the importance of effective environmental and heritage management and conforming to the EMP controls;
(e) ensuring environmental and heritage incidents are managed and closed out;
(f) promoting continual improvement in environmental and heritage management for the duration of the work under the Contract; and
(g) ensure that all Workers, Short Term Workers and Visitors are aware of their environmental and heritage roles and responsibilities.
	EMR Responsibilities

	[bookmark: _Toc214962354]204.22	Training and Competency
	

	1. The Contractor must develop contract-specific environmental induction training that includes as a minimum:
(a) specific environmental responsibilities for all persons and how those responsibilities will be coordinated;
(b) significant Environmental and Heritage Impacts associated with work under the Contract;
(c) specific controls which have been developed to avoid, mitigate and minimise Environmental and Heritage Impacts;
(d) pegging and/or flagging colours used within the Limits of Activity area;
(e) examples of potential environmental and heritage incidents the requirements for reporting environmental incidents; and
(f) a written assessment to be retained under the Contractor’s document management system.
	Contract- specific Induction Training

	2. The Contractor must provide a copy of the environmental induction package to the Superintendent, for approval by the Principal, no less than 14 days prior to the intended start date of physical work under the Contract.
	HOLD POINT

	3. The environmental induction must be undertaken by all Workers and Short Term Workers, including subcontractors, the Superintendent and its agents, and all visitors not fully escorted on Site by inducted persons, prior to commencing physical work under the Contract.
	

	4. The Contractor must evaluate all persons undertaking the environmental induction through a documented competency assessment to ensure that inductees understand the environmental requirements for the Contract.
	Competency Evaluation


	5. The Contractor must not allow Workers to commence physical work under the Contract until they have successfully completed the competency assessment.
	

	6. The Contractor must keep the induction, pre-start and toolbox information up to date with any changes to the scope, risk or Operational Controls of work under the Contract.
	

	7. Prior to the commencement of daily activities, relevant environmental and heritage matters must be clearly communicated during pre-start meetings.
	

	8. The Contractor must retain records of all Workers, Short Term Workers and Visitors who have completed the environmental induction and undertaken the competency assessment.
	

	9. The Contractor must present toolbox presentations to Workers about contract-specific environmental and heritage topics on a regular basis.
	

	[bookmark: _Toc214962355]204.23	Communication
	

	1. Upon approval of the EMP by the Superintendent, the Contractor must ensure the EMP is communicated to all Workers and also must ensure the EMP is:
(a) provided to any Worker upon request;
(b) understood by all Workers (including through the provision of an induction);
(c) communicated to Workers when a change has been made to the EMP; and
(d) is made available for inspection upon request by any Worker, the Superintendent, nominated Superintendent’s staff, auditor or any inspector.
	

	1. The Contractor must have procedures in the EMP for internal communication of environmental information to Workers to ensure they are aware of processes to minimise impacts of the work under the Contract.
	Internal Communication

	1. All external communication to Regulators must be completed by the Principal.  Communication to interested parties must be approved by the Principal prior to the communication occurring.
	External Communication

	[bookmark: _Toc214962356]204.24	Documentation
	

	1. The Contractor must maintain a controlled copy of all Contract environmental documentation on Site.
	Contract Environmental Documentation

	1. [bookmark: _Hlk213747391]Where the EMP references other documentation, these references must be explicit and unambiguous.  The Contractor must ensure that section and clause numbers are clearly denoted in the EMP.  All documentation referenced in the EMP must be available on Site for the duration of the Contract.
	
EMP

	1. The EMP must address all the work under the Contract.
	

	1. The EMR must review and approve in writing all documentation produced by subcontractors, regarding operational controls, to ensure compliance with the EMP prior to the subcontractor commencing any work under the Contract.
	

	1. The Contractor must communicate the EMP to all Workers and any relevant Principal’s personnel approved by the Superintendent.
	Communicate Plan Revision

	1. The Control of documents and the Control of Records must be in accordance with Specification 201 QUALITY MANAGEMENT.
	Control of Records

	[bookmark: _Toc214962357]204.25	Environmental Operational Controls
	

	1. All activities related to the work under the Contract must be contained within the Limits of Activity.
	Limits of Activity

	The Contractor must have Operational Controls to address requirements in Specification 204B and detail them in the EMP.
	

	The Contractor must establish, implement and maintain the Operational Controls to appropriately manage the Risks and Opportunities identified.
	

	Where the Contractor intends to utilise standard procedures and work practices as part of Operational Controls for identified impacts, they must be documented in the EMP.
	

	The Contractor must establish, implement and maintain procedures to ensure that Operational Controls are evaluated and amended, as required.  The evaluation procedure must detail the responsibilities, timelines and records that will be kept as part of the process.
	Evaluation

	The Contractor must ensure Operational Controls are:
(a) clearly documented and those personnel responsible for implementation and management are explicitly defined;
(b) understood by all relevant personnel through training and assessment;
(c) implemented as documented and promptly reviewed for effectiveness following initial implementation;
(d) amended and authorised as required;
(e) adequately supervised, managed and audited to ensure continuing compliance; and
(f) always available wherever the measures are being implemented.
	Operational Controls

	[bookmark: _Toc214962358]204.26	NOT USED
	

	[bookmark: _Toc214962359]204.27	Emergency Management Plan
	

	1. The Contractor must ensure that their Emergency Management Plan prepared in accordance with Specification 203 HEALTH AND SAFETY MANAGEMENT, includes management of environmental and heritage emergencies.
	Emergency Management Plan

	[bookmark: _Toc214962360]204.28	Environmental and Heritage Incidents
	

	1. The EMP must detail who will be responsible for notifying, reporting and submitting environmental and heritage incident notifications to the Principal.
	Notification

	1. The Superintendent must be notified as soon as practicable of all environmental and heritage incidents associated with work under the Contract.
	

	1. The Contractor will be advised by the Superintendent if EQSafe is to be used for the reporting of incidents.
	EQSafe

	1. If EQSafe is not available, the Contractor must use the forms from the Main Roads website, or any updated versions as advised by the Superintendent for all environmental reporting required under the Contract.  The Environment Incident Reporting Form is obtained from the Main Roads website at: https://www.mainroads.wa.gov.au/technical-commercial/contracting-to-main-roads/environmental-heritage-management/
	Environmental Incident Reporting Form

	1. The Contractor must submit a report within twenty-four (24) hours of a moderate, major or catastrophic incident becoming known to the incident reporter.  The Contractor will provide copies of all reports and information associated with the incident to the Superintendent.
	Reporting Timeframe

	1. The Contractor must submit a report within three (3) days of an insignificant or minor incident becoming known to the incident reporter.  The Contractor will provide copies of all reports and information associated with the incident to the Superintendent.
	

	1. The Superintendent may issue actions to be undertaken by the Contractor as a result of an incident.
	Actions

	1. The Contractor must undertake and complete an Environmental Incident Investigation and produce a report to the agreement of the Superintendent for Serious incidents (as defined in Specification 203 HEALTH AND SAFETY MANAGEMENT) within 28 days from notification of the incident.
	Contractor’s Environmental Investigation

	1. In addition to the Contractor’s Environmental Investigation, the Principal may also undertake an investigation into the incident and the Contractor must cooperate with and provide assistance to the investigation as requested by the Superintendent.
	Principal’s Environmental Investigation

	[bookmark: _Toc214962361]204.29 – 204.30	NOT USED
	

	[bookmark: _Toc214962362]MEASUREMENT AND EVALUATION
	

	[bookmark: _Toc214962363]204.31	Monitoring and Measurement
	

	1. The Contractor must establish, implement and maintain procedures for monitoring and measurement of environmental and heritage requirements, and keep records for monitoring and measuring their environmental and heritage performance.
	Monitoring Records

	1. The Construction and Maintenance Monthly Performance Reporting Form must be completed and submitted to the Superintendent within five (5) days of the end of each month.  The form is available on the Main Roads website at https://www.mainroads.wa.gov.au/technical-commercial/contracting-to-main-roads/contractor-reporting/
	Monthly Performance  Reporting Form

	1. Where Contractor Reporting Forms are digitally available via the Construction and Maintenance Portal, the Contractor will report their monthly performance data using the portal.
	

	1. The Contractor must establish, implement and maintain a documented procedure(s) for periodically evaluating compliance with relevant environmental legislation, regulations and other requirements.  The Contractor must keep records of the results of these evaluations.
	Environmental Compliance

	[bookmark: _Toc214962364]204.32	Compliance Auditing
	

	1. The Superintendent may conduct compliance auditing at any time during the Contract.  The Contractor must allow the auditor to conduct the audit on any aspect(s) of this specification.
	Audit

	1. The Contractor must make available at the site suitable facilities to accommodate an auditor, in accordance with Specification 203 HEALTH AND SAFETY MANAGEMENT.
	

	1. The Contractor must develop and maintain an Audit Schedule in accordance with Specification 201 QUALITY MANAGEMENT.  The Audit Schedule must include audits on the effectiveness of the Operational Controls in the EMP.
	Audit Schedule 

	1. The Contractor must implement its approved Audit Schedule and produce a documented report for each audit.  The audit report must detail the audit scope, criteria and findings.  The Superintendent must be provided with the completed audit reports and supporting documentation to show all matters raised have been appropriately addressed.
	Audit Reports

	1. [bookmark: _Hlk213747911][bookmark: _Hlk213747956]Unless otherwise directed by the Superintendent, the Contractor must undertake an initial environmental audit in the first month after work under the Contract has commenced.  The Contractor must undertake subsequent Environmental Audits at a frequency not less than once every three (3) months.
	Minimum Audit Frequency

	[bookmark: _Toc214962365]204.33	Non-conformance and Corrective and Preventative Action
	

	1. Detected non-conformances must be managed in accordance with the requirements of Specification 201 QUALITY MANAGEMENT for the Control of Non-Conforming Output.
	Non-conformances

	1. Corrective and preventative actions must be managed in accordance with the requirements of Specification 201 QUALITY MANAGEMENT.
	Corrective and Preventative Actions

	[bookmark: _Toc214962366]204.34 – 204.40	NOT USED
	

	[bookmark: _Toc214962367]MANAGEMENT REVIEW
	

	[bookmark: _Toc214962368]204.41	Revision of the Environmental Management Plan
	

	1. The EMR, with others as appropriate, must undertake a review of the EMP on a three monthly basis to ensure the EMP remains up to date.  In addition, the Contractor must review and update the EMP where:
(a) there are changes to the scope of work under the Contract;
(b) a non-compliance from compliance auditing has identified deficiencies in the EMP;
(c) a change of Site EMR;
(d) additional Impacts or risks not covered in the EMP are identified; 
(e) a moderate, major or catastrophic environmental incident has occurred; or
(f) where directed by the Superintendent. 
	Review and Revision

	1. Where the EMP has been revised and updated, it must be submitted to the Superintendent for approval within seven days or within a timeframe that is specified by the Superintendent.  
	

	1. The review must include consideration of:
(a) changes in environmental risks and opportunities;
(b) information on the contractor’s environmental performance;
(c) environmental incidents;
(d) audit results;
(e) resources;
(f) relevant communication from interested parties including complaints; and
(g) opportunities for continual improvement.
	

	1. Following the review of the EMP after a non-conformance audit finding or a moderate, major or catastrophic incident, the Contractor must submit a written report that details the suitability, adequacy and effectiveness of the EMP.
	

	[bookmark: _Toc214962369]204.42	Continual Improvement
	

	1. The Contractor must determine opportunities for continual improvement through the management review process and capture these in the EMP.
	

	[bookmark: _Toc214962370]204.43 – 204.80	NOT USED
	

	[bookmark: _Toc214962371]AS-BUILT AND HANDOVER REQUIREMENTS
	

	[bookmark: _Toc214962372]204.81	Handover Requirements
	

	1. The Contractor’s handover requirements are detailed in Annexure 204B.16.
	

	[bookmark: _Toc214962373]204.82 – 204.90	NOT USED
	

	[bookmark: _Toc214962374]CONTRACT SPECIFIC REQUIREMENTS
	

	[bookmark: _Toc214962375]204.91 – 204.99	NOT USED
	




[bookmark: _Toc214962376]ANNEXURE 204A
[bookmark: _Toc214962377]Environmental Management Plan
Construction Environmental Management Plan Template (CEMP)
Construction Environmental Management Plan (CEMP) is the template supplied by the Principal that details the minimum environmental and heritage requirements that the Contractor is to address.  The Contractor must use and populate the CEMP template for work under the Contract.  
Maintenance Environmental Management Plan Template (MEMP)
Maintenance Environmental Management Plan (MEMP) means the template supplied by the Principal that details the minimum environmental and heritage requirements that the Contractor is to address.  The Contractor must use and populate the MEMP template for work under the Contract.
Principal Environmental Work Requirements (PEWR)
Principal Environmental Works Requirements (PEWR) means a document supplied by the Principal that details the minimum environmental and heritage requirements for low risk and low complexity works.  Where a PEWR is provided by the Principal, the Contractor is not required to develop an EMP, but instead comply with, and sign-on to, the controls listed in the PEWR.

GUIDANCE ON WHICH CEMP OR MEMP TEMPLATE OR PEWR TO SELECT IS IN THE GUIDANCE NOTES AT THE END OF THIS DOCUMENT.
ENSURE THAT THE CEMP OR MEMP TEMPLATE OR PEWR <INSERT TRIM REFERENCE> IS INCLUDED AS PART OF THIS SPECIFICATION.



[bookmark: _Toc214962378]ANNEXURE 204B
[bookmark: _Toc214962379]Principal’s Standard and Contract Specific Environmental and Heritage Management Requirements
IF ALL INFORMATION RELATING TO A CLAUSE  IS NOT APPLICABLE, INSERT “NOT USED” AFTER THE HEADING AND DELETE ALL TEXT AND TABLES FROM THE CLAUSE.
204B.1	ABORIGINAL CULTURAL HERITAGE
204B.1.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must develop Operational Controls to address the potential discovery of Aboriginal Cultural Heritage during the Works to ensure any unauthorised impact is avoided.
During site work under the Contract
(b) If suspected human skeletal material is uncovered, the Contractor must:
(i) immediately cease all work within 50 metres of the uncovered material and create an exclusion zone;
(ii) ensure the remains say in-situ and undisturbed;
(iii) immediately report the incident to Police;
(iv) immediately notify the Superintendent;
(v) protect the exclusion zone from any further disturbance and exclude all personnel from the exclusion zone until investigations are completed; and, demarcate the exclusion zone in accordance with Clause 204B.24 Pegging and Flagging.
(c) [bookmark: _Hlk198710433]If suspected Aboriginal Cultural Heritage is uncovered, the Contractor must cease works within 50 metres of the area, create an exclusion zone and notify the Superintendent.  The Superintendent will advise the Contractor of the required actions to be undertaken.
(d) The Contractor must review the EMP to ensure the Aboriginal Cultural Heritage will be adequately managed in accordance with regulatory requirements.
(e) The Contractor must not recommence work under the Contract in the exclusion zone until written approval to proceed is received from the Superintendent.  This is a HOLD POINT.
Post site work 
(f) If relevant, remove bunting that was erected around the exclusion zone.
204B.1.2 Contract Specific Management Requirements
	ABORIGINAL CULTURAL HERITAGE
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) The Contractor must demarcate Aboriginal Cultural Heritage identified in Clause 204B.1.3, in accordance with Clause 204B.28 Special Environment Areas (OR if requested by an Aboriginal group demarcate by using black/pink tape), prior to commencing work under the Contract.
	HOLD POINT

	(b) The Contractor must provide the Principal with a minimum of 3 weeks’ notice prior to the commencement of any earthworks or vegetation clearing activity that requires the attendance of Monitors.
	

	(c) If a Traditional Owner initiated cultural smoking ceremony is required prior to the commencement of the work under the Contract, the Contractor will ensure the risk of fire is mitigated in accordance with Specification 203 HEALTH AND SAFETY MANAGEMENT and Minimum WHS Control Standards.
	

	(d) The Contractor must ensure that the risk of causing adverse Environmental and Heritage Impacts to the Aboriginal Cultural Heritage listed in Clause 204B.1.3 is avoided.
	

	(e) The Contractor must accommodate the presence of Aboriginal Heritage Monitor/s on site in a safe location either by escorting Aboriginal Heritage Monitors or implementing a construction exclusion zone (or enclave area) safe from interaction with construction activities, from which the Aboriginal Heritage Monitors can adequately view the work involving ground disturbance.
	HOLD POINT

	(f) The Contractor must have appropriate PPE available for the Aboriginal Heritage Monitors to use.
	

	(g) Insert Text from Section 18 or Heritage Agreement, which contains the compliance requirements from the Heritage Approvals, etc.
	


204B.1.3 Aboriginal Cultural Heritage Demarcated Area
	LOCATION
	REFERENCE

	(e.g. Drawing Number, Shapefile, Clearing Map)
If this is in the SEA drawing refer to the SEA Drawing Number for the works.
Section 18, Heritage Management Plan or Heritage Agreement avoidance area.
DELETE THIS ROW
	i.e. if there are specific things from the design that need to be mentioned.
i.e. Site to be pegged in accordance with the 201928-0001-construction-peg-colour-code-drawing.pdf (mainroads.wa.gov.au) and the Construction Surveying Guideline.

	
	


204B.1.4 Aboriginal Heritage Act 1972 Section 18 Approval Area OR Heritage Management Plan OR Heritage Agreement Approval Area
	LOCATION
	REFERENCE

	(e.g. Drawing Number, Shapefile, Clearing Map)
Area that the Section 18 / Reg 7/10 covers (potentially whole project site)
DELETE THIS ROW
	i.e. if there are specific things from the design that need to be mentioned.

	
	



204B.2	ACID SULFATE SOILS
204B.2.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor will develop and implement Operational Controls to address the potential discovery of Acid Sulfate Soils (ASS) during work under the Contract, to minimise impacts on the environment.
During site work under the Contract
(b) The Contractor must minimise disturbance below the water table.
(c) The Contractor must avoid activities that have the potential to disturb ASS, either directly, or by affecting the elevation of the water table.
(d) If ASS is uncovered unexpectedly during the work under the Contract, the Contractor must cease work activities and immediately notify the Superintendent.
(e) If there is no existing management plan that adequately addresses the management of ASS, to the Superintendents satisfaction, the Contractor must prepare and implement an ASS Management Plan, in accordance with the Department of Water and Environmental Regulation (DWER) ASS Guideline.
(f) The Contractor will demarcate the unexpected ASS area in accordance with Clause 204B.28 Special Environmental Areas.
Post site work 
(g) The Contractor will remove the demarcation from around the ASS area.
(h) The Contractor will provide the relevant compliance records to the Superintendent.
204B.2.2 Contract Specific Management Requirements
	ACID SULFATE SOILS
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) The Contractor must demarcate the area prior to commencement of site work under the Contract and avoid the area, in accordance with Clause 204B.28 Special Environment Areas.
	

	(b) The Contractor must avoid the actual or potential ASS demarcated area in Clause 204B.2.3. or where the disturbance of ASS is unavoidable, the most appropriate management strategy for the site will be developed prior to disturbance, with approval from the Superintendent.
	

	(c) The Contractor must minimise disturbance and oxidisation of the soil.
	

	(d) The Contractor is responsible for treatment and management of soil and water in ASS within the Limits of Activity area which must be in accordance with DWER’s ASS Guideline to effectively manage potential impacts.
	

	(e) For activities that have the potential to disturb ASS, the Contractor must prepare an ASS Management Plan, prior to disturbance of the actual or potential ASS, using the most appropriate management techniques in accordance with the DWER ASS Guideline.  The ASSMP must be implemented.
	WITNESS POINT

	(f) If > 100m3 of ASS needs to be disturbed, comprehensive Operational Controls must be implemented based on the level of risk associated with the disturbance.
	

	(g) The ASS Management Plan must be prepared to the satisfaction of the Superintendent (with advice from the Principal) prior to the commencement of works in the vicinity of actual or potential ASS.
	HOLD POINT

	(h) The approved ASS Management Plan must be implemented.
	

	(i) The Contractor must maintain records of management and treatment of ASS and provide records and reports to the Superintendent, as specified by the Superintendent.
	

	(j) Post construction activities of the Site will include remediation and validation of the ground surface, including where treatment occurred and associated infrastructure was placed.
	

	(k) Insert specific requirements from Main Roads Acid Sulphate Soil factsheet.
	


204B.2.3 Acid Sulphate Known Locations
	LOCATION
	REFERENCE

	(e.g. Drawing Number, Shapefile, Clearing Map)
DELETE THIS ROW
	i.e. specific elements from the drawing that need to be detailed.
Contaminated/Asbestos/Acid Sulphate sites drawing

	
	



204B.3	CONTRACTOR’S SITE FACILITIES
204B.3.1 Standard Management Requirements
For the purpose of this clause, Site Facilities shall be defined as the facilities necessary for the Contractor to provide in accordance with Specification 100 GENERAL REQUIREMENTS, Clause 103.01(1).
Pre site work under the Contract
(a) The Contractor must submit to the Superintendent for approval the proposed identified locations for Contractor’s Site Facilities that are within the Limits of Vegetation Clearing or are within a previously cleared location within the Limits of Activity.  Evidence of approval from the Superintendent is a HOLD POINT (in accordance with Specification 100 GENERAL REQUIREMENTS).
(b) No native vegetation clearing shall be permitted unless within the Limits of Vegetation Clearing.
(c) The Contractor will ensure Site Facilities are located 50 m away from a watercourse, wetland, well head protection zone or Aboriginal Cultural Heritage area.
(d) The Contractor must include site layout in the EMP.  This figure needs to clearly identify locations of all Site Facilities and must be located within the Limits of Vegetation Clearing and within the Limits of Activity.
During site work under the Contract
(e) The Contractor will ensure that the ablutions are installed and maintained in accordance with the manufacturer’s instructions.
(f) The Contractor must undertake regular monitoring of ablutions to ensure they are in good working order.
(g) The Contractor will ensure that spill response kits are located and maintained on Site and are able to contain spills that may occur at all locations including Contractor’s Site Facilities.
(h) The Contractor will ensure vehicle movements do not disturb vegetation and vehicle turnarounds are limited to Designated Areas.
Post site work 
(i) The Contractor will ensure remediation and reestablishment of the ground surface where Site Facilities were placed to the condition prior to the placement of the Site Facilities.
204B.3.2 Contract Specific Management Requirements
	CONTRACTOR’S SITE FACILITIES
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) The Contractor will ensure that the camp/site office areas are revegetated in line with Specification 304, as applicable.
	

	(b) Insert text from Specification 100 or 304 if necessary.
	



204B.4	CLEARING
204B.4.1 Standard Management Requirements
Refer to Specification 301 VEGETATION CLEARING AND DEMOLITION.
204B.4.2 Contract Specific Management Requirements
	CLEARING
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) All clearing activities must be contained within the Limits of Activity.
	

	(b) The Contractor shall engage a qualified surveyor to clearly and accurately demarcate the Limits of Vegetation Clearing, any trees to be removed/retained and any Special Environmental Areas (SEAs) prior to commencement of clearing.
	HOLD POINT

	(c) If using CPS 818: Prior to leaving the Site, all vehicles, machinery, equipment and plant must be inspected using the Main Roads Hygiene Checklist (available at https://www.mainroads.wa.gov.au/technical-commercial/contracting-to-main-roads/environmental-heritage-management/) to ensure that they are free of soil and vegetation, particularly on tread, tyres, mud flaps and underbody.  Completed checklists are to be retained and provided in the Contractor Reporting specified by the Contract.
	

	(d) If using CPS 818: The Contractor must ensure that clearing of native vegetation is only undertaken in dry conditions, unless otherwise approved and/or directed by the Superintendent.
	

	(e) No additional vegetation shall be cleared without prior approval from the Superintendent.
	HOLD POINT

	(f) The Contractor must clearly communicate and reiterate project pegging and flagging colours in Contract specific site inductions, pre-start meetings, Job Hazard Analysis (JHA), and standard operating procedures.
	

	(g) All clearing of vegetation must be reported to the Superintendent as part of the Contract Reporting under the Contract.
	

	(h) Insert Contractor requirements from CPS 818 (particularly if the clearing is at variance to the Principles), Project Specific Clearing Permit, Part IV Ministerial Statement or EPBC Approval clearing that are additional to standard management requirements.
	



204B.5	COMMUNICATION
204B.5.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor will ensure Operational Controls, environmental risks and Special Environmental Areas are communicated to all Workers, Short Term Workers and Visitors prior to commencing works.
During site work under the Contract
(b) The Contractor will ensure Operational Controls are communicated through contract specific site inductions, pre-starts, toolbox meetings, procedures and processes.
(c) External environmental communication to Regulators will be conducted by the Principal.
Post site work 
(d) Nil.
204B.5.2 Contract Specific Management Requirements
	COMMUNICATION
	HOLD / WITNESS POINT

	Nil.
(OR delete this row and amend requirements below as applicable, change text to black)
	

	(a) Insert text from Stakeholder Management Plan and/or Land Owner Communication Commitments.
	



204B.6	CONTAMINATION
204B.6.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor will develop and implement Operational Controls to address the potential discovery of contamination during work under the Contract, to minimise Environmental and Heritage Impacts.
During site work under the Contract
(b) If during the work under the Contract, the Contractor causes a site to become contaminated, the Contractor shall be responsible for rehabilitating the area, at their own expense, in accordance with regulatory requirements and the Contractor’s procedures, to the written approval of the Superintendent.  This is a HOLD POINT.
(c) All contaminated materials must be disposed of as soon as practicable at a designated location approved by the Superintendent.
(d) If an unexpected contaminated area is uncovered during the works and there are no Operational Controls to adequately minimise the impact, the Contractor must:
(i) immediately cease all work within 10 metres of the unexpected contaminated area;
(ii) immediately notify the Superintendent;
(iii) protect the unexpected contaminated area from any further disturbance and exclude all Workers, Short Term Works and Visitors from the site until investigations are completed, unless they are associated with the investigation;
(iv) demarcate the unexpected contaminated area in accordance with Clause 204B.28 Special Environment Areas; and
(v) not recommence works in the demarcated unexpected contaminated area until written approval to proceed is received from the Superintendent.  This is a HOLD POINT.
(e) The Superintendent will advise the Contractor if the unexpected contaminated area has been reported to the Regulator.
(f) The Contractor must review their risk assessment and review the Operational Controls to ensure the unexpected contaminated area will be adequately managed in accordance with Regulator’s requirements.
(g) The Contractor must obtain Superintendent approval of the revised EMP prior to recommencing works within proximity of the unexpected contaminated area. 
Post site work 
(h) The Contractor must supply relevant compliance records to the Superintendent.
(i) The Contractor will either remove the demarcation at the completion of the works and/or erect signage in the area, where directed by the Superintendent.
204B.6.2 Contract Specific Management Requirements
	CONTAMINATION
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) The Contractor will ensure contaminated sites are demarcated, in accordance with Clause 204B.28 Special Environment Areas, prior to works commencing.
	

	(b) The Contractor must avoid disturbance to the demarcated contaminated areas in Clause 204B.6.3.
	

	(c) Where disturbance of contamination areas is unavoidable, the Contractor will arrange a Preliminary Site Investigation (PSI) to be completed by a certified professional, prior to disturbance in accordance with DWER’s Guideline on Assessment and management of contaminated sites.
	

	(d) If the site investigation identifies contamination, the Contractor must develop a Conceptual Site Model (CSM), in accordance with the DWER Guideline, to the satisfaction of the Superintendent, prior to commencing site work under the Contract in that area.
	

	(e) Where a Contaminated Sites Management Plan is required to be developed by the Contractor, the Contractor must ensure that the management actions are prepared to the approval of the Superintendent.
	

	(f) The Contractor must develop and implement Operational Controls and procedures to manage the contamination and identified risks, as advised by a certified professional.
	

	(g) The Contractor must maintain records of compliance with the management measures and provide records and reports to the Superintendent on request.
	

	(h) Insert commitments from a Contaminated Site Management Plan.
	


204B.6.3 Known Contaminated Site Locations
	LOCATION
	REFERENCE

	(e.g. Drawing Number, Shapefile, Clearing Map)
ASS and CS Presentation Drawing Environmental Factsheet in development @ D23#729911)
DELETE THIS ROW
	i.e. Drawing number

	
	



204B.7	DEWATERING
204B.7.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must determine if dewatering activities require a 5C groundwater or surface water licence or are exempt from a water licence.
(b) The Contractor must provide documented evidence to the Superintendent showing that a licence is/is not required prior to the commencement of dewatering activities.
(c) The Contractor must develop processes to ensure compliance with licence conditions or exemption thresholds.
(d) The location where dewatering water is proposed to be discharged or stored, shall be approved by the Superintendent prior to the commencement of dewatering.
During site work under the Contract
(e) The Contractor must ensure dewatering activities are carried out in accordance with the conditions of any licences or that dewatering activities continue to meet the requirements that provide an exemption (i.e. not exceeding 10 L/second over a period of less than 30 consecutive days and the total volume of water taken over the period does not exceed 25,000 kilolitres).
(f) The Contractor must avoid extracting contaminated groundwater, wherever possible.
(g) The Contractor must ensure all water extracted will be discharged or stored in a manner consistent with the guidance provided in Water Quality Protection Notes (WQPN) 13 – Dewatering of soils at construction sites, and approved by the Superintendent.
(h) The Contractor is required to document dewatering activity including dates of dewatering, volumes of dewatering and any water quality information requested in WQPN 13 and submitted to the Superintendent as part of the Contractor Reporting specified by the Contract.
(i) If dewatering activities causes turbidity, sedimentation or erosion of a waterway or drainage line, the Contractor will implement appropriate measures to mitigate the impacts prior to discharge, or the dewatering volume/rate will be decreased, as approved by the Superintendent.
Post site work 
(j) All dewatering equipment will be removed from site as soon as possible after dewatering ceases.
(k) The Contractor must provide dewatering and disposal records to the Superintendent.

204B.7.2 Contract Specific Management Requirements
	DEWATERING
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) The work under the Contract is located within a proclaimed ground water area and requires the Contractor to conduct specific water testing and establish buffer zones, prior to works commencing.
	

	(b) The Contractor may be required to determine the water quality, prior to dewatering, as advised by the Superintendent.
	WITNESS POINT

	(c) The Contractor must prepare a Dewatering Management Plan prior to commencing dewatering activity, for the approval of the Superintendent.
	WITNESS POINT

	(d) Insert text from Dewatering licence or measures required in a proclaimed water area.
	



204B.8	DEMOLITION
204B.8.1 Standard Management Requirements
Refer to Clause 301.17 Demolition in Specification 301 VEGETATION CLEARING AND DEMOLITION.
Pre site work under the Contract
Nil.
During site work under the Contract
(a) Existing features must be demolished either to the extent as shown on the Drawings or as otherwise detailed in Annexure 301B.  Demolition work includes the removal of existing non-vegetative material such as but not limited to kerbing, pipes, rubbish, site debris, and the like.
Post site work 
Nil.
204B.8.2 Contract Specific Management Requirements
	DEMOLITION
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) The Contractor must ensure waste and dust from demotion works is properly contained, managed and disposed of in accordance with environmental regulations and site safety requirements.
	



204B.9	DIEBACK MANAGEMENT
204B.9.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must ensure the risk of spreading dieback and causing adverse impacts to the environment is avoided and/or minimised as low as practicable.
(b) The Contractor must demarcate any dieback areas in accordance with Clause 204B.28 Special Environmental Areas. This is a HOLD POINT.
(c) The Contractor must ensure a hygiene check and brush down and/or wash down of vehicles, machinery, equipment, and plant is conducted prior to being used on Site.
(d) The Contractor must complete the Main Roads Hygiene Checklist (available at https://www.mainroads.wa.gov.au/technical-commercial/contracting-to-main-roads/environmental-heritage-management/), for all vehicles, machinery, equipment and plant prior to being used of Site.
(e) The Contractor must know the origin of all material (soil, mulch, fill, gravel, etc.) prior to the material being brought into a dieback free area, and the material must be known to be from a dieback free location. 
During site work under the Contract
(f) The Contractor must ensure no known dieback infested soil, mulch, fill or other material will be permitted into the Site.
(g) The Contractor must monitor the implementation of dieback Operational Controls through daily visual inspections during clearing activities and record soil movements during wet weather events.
(h) When undertaking clearing, the Contractor must ensure that no soil disturbing activity occurs in dieback infested areas during rain events where there is a risk of transporting dieback into uninfested or uninterpretable areas.
(i) Hygiene Checklists and the Hygiene Inspection Register (if required for vehicles entering a Clean on Entry Point) must be submitted to the Superintendent as part of the Contractor Reporting specified by the Contract.
(j) The Contractor must allow the Principal or Superintendent to inspect at any time, any vehicles, machinery, equipment and plant to verify they have been cleaned down appropriately.
(k) The Contractor must dispose of dieback infested or potentially dieback infested soil in a dieback infested area by burial to at least 300 mm below surface or removal from Site to an appropriate location.  The Superintendent shall approve the proposed disposal location.
Post site work 
(l) The Contractor must ensure all vehicles and machinery are cleaned down and Hygiene Inspection Checklists completed (Main Roads Hygiene Checklist (available at https://www.mainroads.wa.gov.au/technical-commercial/contracting-to-main-roads/environmental-heritage-management/), prior to the vehicles/machinery leaving the project area.
204B.9.2 Contract Specific Management Requirements
	DIEBACK MANAGEMENT
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) The EMR is required to attend Green Card training prior to commencing work under the Contract.
	

	(b) The Contractor must demarcate the dieback areas listed in Clause 204B.9.3 Dieback Infested Locations.
	

	(c) The Contractor must develop and implement a Dieback Management Plan.
	

	(d) If disturbance of the dieback area is unavoidable, the Contractor must establish and install dieback signs for vehicle entry and exit, vehicle hygiene inspection points and storage locations of dieback infested and dieback free materials, prior to the commencement of site work under the Contract and with approval from the Superintendent.
	

	(e) The Contractor must ensure all vehicles, machinery, equipment and plant that are moving between dieback infested and dieback free sites must be inspected at Inspection Points and recorded in the Hygiene Inspection Register (Word document) available at https://www.mainroads.wa.gov.au/technical-commercial/contracting-to-main-roads/.
	

	(f) If the Contractor must strip dieback infested topsoil and store on site, it must be stored in accordance with Drawing (201928-0011-1) and must be signposted in accordance with 201928-0007 – Construction Environmental Management Signs.
	

	(g) The Contractor must ensure dieback infested stockpiles will be disposed of/buried in a dieback infested area in a location approved by the Superintendent.
	

	(h) The Contractor must provide copies of all completed Hygiene Inspection Registers (if required) within fourteen (14) business days of Practical Completion.
	

	(i) Insert text from site-specific Dieback Management Plan.
	


204B.9.3 Dieback Infested, Dieback Uninterpretable, and Dieback Free Locations
	LOCATION
	REFERENCE

	(e.g. Drawing Number, Shapefile, Clearing Map)
Dieback drawings
DELETE THIS ROW
	i.e. specific elements from the design that need to be detailed.

	
	



204B.10	DOCUMENTATION MANAGEMENT
204B.10.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must prominently display Main Roads Environmental Policy on a site office notice board for the duration of the Contract and include it in information provided to all personnel.
During site work under the Contract
(b) The Contractor must establish, implement and maintain procedures to ensure Operational Controls are evaluated and amended as required.  The evaluation procedure/s must detail responsibilities, timelines and records that will be kept as part of the process.
(c) Following an amendment to the EMP during work under the Contract, the Contractor must ensure the Operational Controls are in accordance with the Contract and must re-submit the EMP to the Superintendent for approval within 10 business days of amendments being made.
(d) The Contractor must be responsible for ensuring subcontractor compliance with the approved EMP and the maintenance of records to demonstrate subcontractor compliance.
Post site work 
(e) The Contractor must provide relevant environmental and heritage records to the Superintendent within 14 days of the Date of Practical Completion.
204B.10.2 Contract Specific Management Requirements
	DOCUMENTATION MANAGEMENT
	HOLD / WITNESS POINT

	Nil.
(OR delete this row and amend requirements below as applicable, change text to black)
	

	(a) Insert text regarding specific documentation for environmental requirements.
	



204B.11	DUST (FUGITIVE) MANAGEMENT
204B.11.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must identify the sources and activities of the work under the Contract that have the potential to generate dust and cause adverse impacts to community amenity and the environment.
(b) The Contractor must have Operational Controls in relation to dust in place prior to conducting activities that have the potential to generate dust.
(c) If dust suppression using water is an Operational Control, the water source must be identified prior to the commencement of site work under the Contract and be from a source approved by the Superintendent (in accordance with Specification 303 MATERIALS AND WATER SOURCES).
During site work under the Contract
(d) The Contractor must ensure where storing, handling or transporting material that has the potential to cause dust emissions, material is covered, treated and/or dampened.
(e) The Contractor must ensure that construction methods keep dust emissions to a minimum, particularly during clearing and earth moving activities.
(f) The Contractor must ensure dust emissions are visually monitored during the Works to ensure the Operational Controls in place are effective in controlling dust emissions.
(g) The Contractor must ensure that vegetation is only cleared when necessary and during conditions that minimise dust emissions.
(h) The Contractor must ensure that areas requiring soil stabilisation, or areas subject to wind erosion, are treated as soon as practicable to minimise dust emissions.
(i) If Operational Controls for dust are found to be insufficient, then the Contractor shall enhance Operational Controls as approved by the Superintendent.
Post site work 
Nil.
204B.11.2 Contract Specific Management Requirements
	DUST (FUGITIVE) MANAGEMENT
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) If saline/nutrient rich water is being used for dust suppression, the Contractor must conduct regular monitoring of vegetation health to ensure no decline to vegetation from the saline/nutrient rich water.  The frequency of vegetation monitoring is required to be monthly for early recognition of vegetation health indicators.
	

	(b) The Contractor must immediately communicate any changes in vegetation health condition to the Supervisor to enact changes to onsite practices.
	

	(c) Insert text of dust control requirements from project specific approvals or if asbestos or contaminated site is present.
	



204B.12	EROSION AND SEDIMENTATION CONTROL
204B.12.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must ensure material stockpiles are located at least 50 m away from open drainage lines and natural waterways, and/or outside of potential flood risk areas, prior to the commencement of site work under the Contract.
(b) The Contractor must ensure drainage lines and natural waterways are not obstructed by excavated material.
During site work under the Contract
(c) [bookmark: _Hlk143873122]The Contractor must ensure all recently cleared, exposed and loose surface areas shall be protected from erosion from all sources including, but not limited to, wind, water and soil.
(d) The Contractor must ensure material stockpiles are not susceptible to erosion or have the potential to cause sedimentation.
(e) The Contractor must prevent sedimentation and siltation of waterbodies and drainage lines.
(f) The Contractor must visually monitor erosion and sedimentation during the work under the Contract to ensure soil rills are not forming, and natural drainage pathways, soil fertility, surface water turbidity and infrastructure are not impacted.
(g) The Contractor must inspect the Site and any adjacent lands within 24 hours of a rainfall event that may reasonably result in erosion or transfer of sediment.  The inspection must assess the adequacy of erosion and sedimentation Operational Controls implemented by the Contractor.
(h) If Operational Controls for erosion and sedimentation are found to be insufficient, then the Contractor shall enhance Operational Controls as approved by the Superintendent.
Post site work 
(i) As soon as practicable after site work under the Contract has been completed, the Contractor must ensure areas impacted by erosion and sedimentation, or areas susceptible to erosion and sedimentation by the contracted work, are restored and stabilised to the satisfaction of the Superintendent, so that the soil, natural topography and/or waterways are not susceptible to erosion or sedimentation in the future.
204B.12.2 Contract Specific Management Requirements
	EROSION AND SEDIMENTATION CONTROL
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) The Contractor must install sedimentation fencing, silt curtains and/or geofabric/geotextile liners to minimise Environmental and Heritage Impacts to the waterway.
	

	(b) Insert text that may be required if the site or materials being used are more susceptible to erosion and sedimentation, or near sensitive receptors.
	



204B.13	FAUNA MANAGEMENT
204B.13.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor will develop and implement Operational Controls to minimise the risk of causing adverse impacts to native fauna, their potential breeding sites and habitats during the work under the Contract.
(b) The Contractor must ensure that site personnel are aware of what actions to take to protect native fauna, prior to commencing site work under the Contract.
During site work under the Contract
(c) The Contractor must ensure that all Workers and Short Term Workers undertake visual monitoring and are vigilant to the potential presence of native fauna.
(d) The Contractor must ensure:
(i) no pets, traps or firearms are brought into the project area;
(ii) fauna are not fed;
(iii) fauna are not intentionally harmed or killed; and
(iv) fauna that venture into the work area are encouraged to leave in a manner that does not harm the animal or Workers or Short Term Workers (avoid loud noises, approach slowly).
(e) Where active nests, burrows or dens are identified, site work under the Contract must not proceed until the Contractor obtains the Superintendent’s approval for the management of potential fauna present.
(f) The Contractor must ensure that any required clearing is conducted in a manner to allow fauna to naturally move out of the area by clearing in one direction towards areas of native vegetation that will remain undisturbed.
(g) The Contractor must report fauna injury and/or fatality as a result of the work under the Contract as an Environmental Incident.
(h) The Contractor must ensure that if sick, injured or orphaned native wildlife are located within the Site, the Wildcare Helpline (08 9474 9055), local rehabilitation group, veterinarian or the local government ranger will be contacted for assistance. Records of communication with the wildlife carer must be retained.
Post work 
Nil.
204B.13.2 Contract Specific Management Requirements
	FAUNA MANAGEMENT
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) The Contractor will, prior to the commencement of clearing, use machinery to tap large habitat trees to encourage any animals to evacuate prior to the tree being felled.
	

	(b) The Contractor must keep at least one designated fauna rescue kit onsite.  As a minimum the fauna rescue kit must include towel, protective gloves and a box/container for transporting the animal.
	

	(c) Insert text of fauna management requirements from project specific approvals.
	


204B.13.3 Fauna Habitat Locations
	LOCATION
	REFERENCE

	(e.g. Drawing Number, Shapefile, Fauna Habitat Map)
DELETE THIS ROW
	

	
	



204B.14	FENCING
204B.14.1 Standard Management Requirements
Refer to Specification 903 FENCING.
Pre site work under the Contract
(a) The Contractor must ensure the land owner has been notified prior to commencing fencing works.
(b) Barbed or razor wire will not be used in and adjacent to fauna SEAs.
During site work under the Contract
(c) The Contractor will minimise unnecessary vegetation disturbance and limit damage to neighbouring native vegetation, especially if the fence is in or adjacent to a SEA.
(d) The Contractor will ensure the width of clearing for fencing through native vegetation is minimised as far as practicable and shall not exceed three metres either side of the fence or as directed by the Superintendent.
(e) When maintaining a fence the Contractor will use a chainsaw (hand-held equipment) to minimise the amount of clearing and soil disturbance, and consider if pruning can allow the work under the Contract to proceed without clearing vegetation.
(f) Arrangements shall be made at the Contractor’s own expense, for the removal and disposal of redundant/damaged fencing to an approved disposal location.
Post work 
(g) If a fence has been damaged or impacted during the works, the Contractor will ensure the fence is restored or replaced, and the appearance shall be as close to original as practicable.
(h) The road reserve must be left in a safe and stable condition by the Contractor, to the approval of the Superintendent.
204B.14.2 Contract Specific Management Requirements
	FENCING
	HOLD / WITNESS POINT

	Nil.
(OR delete this row and amend requirements below as applicable, change text to black)
	

	(a) Insert text of fauna management requirements from project specific approvals.
	



204B.15	FIRE MANAGEMENT
Refer to Specification 203 HEALTH AND SAFETY MANAGEMENT.
204B.15.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must ensure there are Operational Controls in place to avoid or minimise the risk of Workers and Short Term Workers or the work under the Contract causing a bush-fire.
During site work under the Contract
(b) The Contractor must ensure that Operational Controls to prevent or minimise bushfire risk are implemented, particularly during activities such as hot works and when machinery with hot exhaust systems operate near dry vegetation.
(c) The Contractor must ensure that all Workers and Short Term Workers conduct visual monitoring and remain vigilant to the risk of bush-fires.
(d) If there is a fire as a result of the work under the Contract and vegetation is burnt, the Contractor must report the fire as an Environmental Incident (as well as a safety incident).
Post work
Nil.
204B.15.2 Contract Specific Management Requirements
	FIRE MANAGEMENT
	HOLD / WITNESS POINT

	Nil.
(OR delete this row and amend requirements below as applicable, change text to black)
	

	(a) Insert text of fire management requirements from project specific approvals.
	



204B.16	HANDOVER REQUIREMENTS
204B.16.1 Standard Management Requirements
Pre site work under the Contract
Nil.
During site work under the Contract
(a) The Contractor must confirm with the Superintendent how the records below will be issued to the Superintendent.
Post work 
(b) Within fourteen (14) business days of the Date of Practical Completion, the Contractor must ensure the following are issued to the Superintendent:
(i) closed out Environmental Incident investigations, corrective actions and audit actions, and
(ii) communications register and evidence of timely response to all environmental complaints.
204B.16.2 Contract Specific Management Requirements
	HANDOVER REQUIREMENTS
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) Where activities have taken place utilising a Department of Biodiversity, Conservation and Attractions permit for work under the Contract in the Swan and Canning River Development Control Areas, the completed close-out report together with all required evidence must be provided to the Superintendent within 14 business days of Date of Practical Completion.
	

	(b) Insert text for project specific handover and practical completion requirements.
	



204B.17	HAZARDOUS MATERIALS
204B.17.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must ensure that the risk of hazardous materials causing Environmental and Heritage Impacts to the community, environment or infrastructure is avoided and/or minimised.
(b) The Contractor must ensure there are Operational Controls to address high-risk activities including, but not limited to:
(i) storage of bitumen, asphalt, concrete or aggregate;
(ii) precoating;
(iii) fuel storage;
(iv) designated areas for refuelling and mobile refuelling locations;
(v) hazardous materials and chemical storage;
(vi) vehicle and machinery minor maintenance and servicing;
(vii) hazardous waste storage and disposal.
(c) The Contractor must nominate the designated location for undertaking all high-risk activities for the Superintendent’s approval and show this on the site layout figure in the EMP.
(d) The Contractor must ensure all hazardous material spills are cleaned up immediately and material is appropriately disposed of in an approved location.  Such spills must be reported and investigated as an Environmental Incident.
(e) The Contractor must ensure that hazardous materials handling and storage are consistent with the relevant Safety Data Sheets.
(f) When storing bulk hazardous materials (including fuel), the Contractor must ensure that infrastructure (including pipelines) must be labelled, signposted or otherwise indicate the contents and be protected from vehicular impact (e.g. earthen windrows, bollards, concrete blocks etc.).
During site work under the Contract
(g) The Contractor must ensure activities involving the handling or storage of hazardous materials are not undertaken within 50 metres of any sensitive receptors including, but not limited to:
(i) watercourses;
(ii) wetlands;
(iii) Public Drinking Water Source Areas (PDWSAs);
(iv) wellhead protection zones;
(v) protected land tenure; or
(vi) Special Environmental Areas (SEAs).
(h) The 50 metre distance referenced in (g) above may be reduced if approved by the Superintendent where the Contractor can demonstrate that the high-risk activities additional Operational Controls are satisfactory to the Superintendent.
(i) The Contractor must ensure that the storage and management of hazardous materials is regularly inspected and maintained.
(j) The Contractor must ensure hazardous materials containment area (bund) is emptied (using vacuum truck or similar) prior to cyclone/extreme weather events and after significant rainfall, and fluid removed from containment area must be regarded as contaminated liquid waste.
Post site work under the Contract
(k) The Contractor must remove all hazardous materials from Site.
(l) The Contractor must ensure that hazardous materials are disposed of at an approved hazardous materials facility.
204B.17.2 Contract Specific Management Requirements
	HAZARDOUS MATERIALS
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) The Contractor must ensure that the volume of hazardous materials stored within 50 metres of the PDWSA and wellhead protection zone, does not exceed the following requirements:
(i) for Priority 1 PDWSAs, less than 200 Litres; and
(ii) for Priority 2 PDWSAs, less than 1000 Litres.
	

	(b) The Contractor must install hydrocarbon booms within the waterway and monitor their effectiveness to minimise the potential impact of hazardous materials on the aquatic environment.
	

	(c) Insert text from project approvals or relevant to sensitive areas within the project area.
	



204B.18	HISTORIC HERITAGE
204B.18.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must develop Operational Controls to address the potential discovery of historic heritage sites during the work under the Contract, to ensure any impact is avoided.
(b) The Contractor must ensure Workers and Short Term Workers are aware of the processes to follow if an unexpected or potential historic heritage site and/or heritage material is uncovered during the work under the Contract.
During site work under the Contract
(c) The Contractor must minimise structural, vibration, dust and water impacts on historical heritage sites including, but not limited to, buildings, structures, features, sites or objects.
(d) If an unexpected or potential historic heritage site is uncovered, the Contractor must:
(i) immediately cease all work within 5 metres of the unexpected or potential historic heritage site and/or material;
(ii) immediately notify the Superintendent;
(iii) protect the unexpected or potential historic heritage site and/or materials from any further disturbance and exclude all Workers and Short Term Works from the location until all investigations are completed; and
(iv) demarcate the area in accordance with Clause 204B.28 Special Environment Areas.
(e) The Superintendent will advise the Contractor of the required actions to be undertaken in response to an unexpected or potential historic heritage site and/or materials.
(f) The Contractor must review Operational Controls to ensure any unexpected historic heritage sites will be adequately managed in accordance with the requirements of the Regulator to prevent deterioration from the work under the Contract.
(g) The Contractor must obtain Superintendent approval if the EMP needs to be revised, prior to recommencing work within proximity of the unexpected historic heritage site. 
(h) The Contractor must not recommence work under the Contract in the demarcated area until the Superintendent has provided written approval to proceed.  This is a HOLD POINT.
Post site work 
(i) The Contractor is to ensure there are no impacts to historical heritage sites resulting from the work under the Contract, and no waste left at historic heritage locations when works are complete.
204B.18.2 Contract Specific Management Requirements
	HISTORIC HERITAGE
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) The Contractor must demarcate historical heritage sites for protection in accordance with Clause 204B.28 Special Environment Areas, prior to commencing site work under the Contract in the area.
	

	(b) The Contractor must protect nominated heritage, cultural and/or social heritage locations listed in Clause 204B.18.3 from impacts during the Works.
	

	(c) At the conclusion of the site work under the Contract, the Contractor is to provide post-construction Property Condition Survey reports for all nominated historic heritage locations and provide to the Superintendent.
	

	(d) Insert text from a site-specific Heritage Management Plan.
	


204B.18.3 Historic Heritage Locations
	LOCATION
	REFERENCE

	(e.g. Drawing Number, Shapefile, Clearing Map)
Heritage, cultural and/or social heritage locations
DELETE THIS ROW
	i.e. specific elements from the design that need to be detailed.

	
	



204B.19	INDUCTIONS, PRE-STARTS AND TOOLBOX TOPICS
204B.19.1 Standard Management Requirements
Refer to Clause 204.22.
204B.19.2 Contract Specific Management Requirements
	INDUCTIONS, PRE-STARTS AND TOOLBOX TOPICS
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) The Contractor will ensure all Workers and Short Term Workers are aware of the Operational Controls that need to be followed if contaminated sites or hazardous materials are identified on site during work under the Contract.
	

	(b) Insert text regarding certain topics from approvals if required to be in the induction or toolbox presentations.
	



204B.20	LAYDOWN AREAS
204B.20.1 Standard Management Requirements
Pre site work under the Contract
(a) For laydown areas which are Contractor nominated, the Contractor must obtain all relevant legislative and land access approvals and provide to the Superintendent for their approval.  Superintendent approval of the laydown areas is a HOLD POINT.
(b) Laydown areas must be within the Limits of Activity.
(c) The Contractor must ensure the extent of the laydown areas are demarcated and access, entry and exit is clearly signposted.
(d) The Contractor is responsible for ensuring all activities conducted at the laydown areas (e.g. machine servicing, waste storage, hazardous chemical storage) have been approved by the Superintendent prior to commencement of the activity.
During site work under the Contract
(e) The Contractor must ensure that activities conducted, and machinery and materials stored at the laydown areas do not cause adverse Environmental and Heritage Impacts.
(f) The Contractor is responsible for ensuring all laydown items and activities occur within the demarcated laydown areas.
(g) The Contractor is responsible for ensuring vehicles, materials and equipment are not stored on native vegetation and not parked/stored up against trees and shrubs, potentially impacting the root zone.
Post work 
(h) All material and spoil stockpiles, flagging, waste, equipment and infrastructure shall be removed at the conclusion of the site work under the Contract.
(i) The laydown areas must be left in a safe and stable condition, rehabilitated and stabilised at the conclusion of the site work under the Contract, to the approval of the Superintendent.
204B.20.2 Contract Specific Management Requirements
	LAYDOWN AREAS
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) The Contractor must confirm to the Superintendent that the laydown areas do not require any clearing of vegetation, including for vehicle parking and turnarounds, and storage activities.
	

	(b) Insert text from project approvals for specific laydown environmental and heritage requirements.
	



204B.21	MACHINERY, PLANT AND VEHICLE MANAGEMENT
204B.21.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must ensure that all areas associated with the storage, parking, servicing, refuelling, clean down, access roads and turn around areas of all vehicles, plant and machinery is located within the Limits of Activity and/or other locations approved by the Superintendent.
(b) The Contractor must ensure all vehicles, plant and machinery are well maintained and fit for purpose prior to commencing site work under the Contract.
During site work under the Contract
(c) The Contractor must ensure only minor servicing and maintenance is undertaken at designated areas within the Site.
(d) All major servicing/maintenance is to be undertaken off Site at an appropriate facility.
(e) The Contractor must ensure vehicle, plant and machinery refuelling is only undertaken at designated areas approved by the Superintendent.
(f) Spill mats or trays must be used during servicing/maintenance and refuelling activities on Site if not undertaken on a hardstand.
Post work 
Nil.
204B.21.2 Contract Specific Management Requirements
	MACHINERY, PLANT AND VEHICLE MANAGEMENT
	HOLD / WITNESS POINT

	Nil.
(OR delete this row and amend requirements below as applicable, change text to black)
	

	(a) Insert text regarding certain requirements from approvals.
	



204B.22	MULCH AND TOPSOIL
204B.22.1 Standard Management Requirements
Pre site work under the Contract
(a) Prior to any clearing commencing, the Contractor must plan for the storage, handling, disposal and/or reuse of any mulch, vegetation and topsoil stockpiles within the Limits of Activity.  The proposed plan must be approved by the Superintendent.
During site work under the Contract
(b) The Contractor must segregate, demarcate and signpost ‘suitable’ materials from ‘contaminated/unsuitable’ materials, for potential respreading at the completion of the site work under the Contract.  ‘Contaminated/unsuitable’ material is weed, dieback, debris or otherwise infested material which would hinder plant growth) (Drawing 201928-0007 – Construction Environmental Management Signs (available at https://www.mainroads.wa.gov.au/technical-commercial/technical-library/).
(c) Stockpiles are to be segregated and signposted in accordance with Drawing 201928-0002 –  Stockpile Cross Sections (available at https://www.mainroads.wa.gov.au/technical-commercial/technical-library/).
(d) The Contractor must ensure ‘suitable’ materials remain ‘clean’ during storage, stockpiling and handling and are not mixed with actually or potentially ‘contaminated/unsuitable’ material without prior approval from the Superintendent.
(e) The Contractor must ensure that ‘suitable’ stockpiles are managed so that the materials are not degraded or made contaminated/unsuitable for use in rehabilitation.
Post work 
(f) The Contractor will ensure no ‘suitable’ stockpiled mulch, vegetation and topsoil remains at the conclusion of the site work under the Contract, and all material has been respread over cleared areas or removed from Site, to a location approved by the Superintendent.
(g) The Contractor will ensure ‘contaminated/unsuitable’ stockpiled material is removed from Site. 
204B.22.2 Contract Specific Management Requirements
	MULCH AND TOPSOIL
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) Where vegetation or mulch is planned to be moved outside of the Limits of Vegetation Clearing, the Contractor must determine, prior to clearing commencing:
(i) if any quarantine zones confine the movement of the vegetation and/or mulch;
(ii) 	if there are any treatments (such as mulch size) that may affect the transporting of vegetation and/or mulch;
(iii) 	if the end location (if a waste/recycling facility, land owner or depot) can confirm it will accept the vegetation and mulch.
	

	(b) Insert text regarding revegetation/landscaping requirements from approvals, or revegetation, rehabilitation or landscaping requirements as per Specification 304.
	



204B.23	NOISE MANAGEMENT
204B.23.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must develop and implement Operational Controls to avoid and/or minimise noise impacts from work under the Contract.
(b) Where work under the Contract is proposed to be undertaken outside the hours of 7am-7pm on any day, or on any Sunday or public holiday, with noise levels anticipated to exceed assigned levels at noise sensitive premises (as defined in Regulation 8 of the Environmental Protection (Noise) Regulations 1997), the Contractor must:
(i) prepare and submit a Noise Management Plan to the appropriate Local Government for review and approval, at least 10 working days prior to the proposed commencement of work under the Contract;
(ii) not commence any work under the Contract which will or may exceed the assigned level defined within the relevant acts and regulations until both Local Government and Superintendent approval is received; and
(iii) implement and comply with the Noise Management Plan.
During site work under the Contract
(c) The Contractor must ensure that the risk of noise from work under the Contract causing Environmental and Heritage Impacts (with particular consideration of the community, fauna and sensitive premises such as residential areas, businesses, hospitals or schools), is avoided and/or minimised, particularly for night works.
(d) The Contractor is responsible for conducting works in accordance with Australian Standard 2436-2010 Guide to noise and vibration control.
(e) Any reversing alarm fitted to a vehicle or plant item associated with the work under the Contract must be a ‘reversing squawker’; except where:
(i) the installation of a ‘reversing squawker’ would cause the Contractor to breach the requirements of the Environmental Protection (Noise) Regulations 1997 (WA); or
(ii) there is a demonstratable work health and safety benefit of utilising a ‘reversing beeper’ or other reversing alarm, as approved by the Superintendent.
(f) The Contractor will record any noise complaints arising from the work under the Contract, report them as an Environmental Incident, and investigate and minimise the Environmental and Heritage Impacts in consultation with the Superintendent.
(g) The Contractor is responsible for resolving all noise complaints in a timely manner, in consultation with the Superintendent.
Post site work 
Nil.
204B.23.2 Contract Specific Management Requirements
	NOISE MANAGEMENT
	HOLD / WITNESS POINT

	Nil.
(OR delete this row and amend requirements below as applicable, change text to black)
	

	(a) Insert text from approvals that may have noise management requirements.
	



204B.24	PEGGING AND FLAGGING
204B.24.1 Standard Management Requirements
Pre site work under the Contract
(a) Prior to all clearing, the Contractor must install pegging and flagging in accordance with the Main Roads Construction Surveying Guideline.  The pegging and flagging must be clearly visible by operators and be the appropriate colour and spacing, in accordance with Drawing 201928-0001-1 Construction Peg Colour Code (available at https://www.mainroads.wa.gov.au/technical-commercial/technical-library/).
(b) All Workers and Short Term Workers must be aware within their Contract specific site inductions that:
(i) white flagging identifies vegetation to be retained;
(ii) pink flagging identifies vegetation to be removed;
(iii) orange rope flagging identifies Special Environmental Areas (SEAs);
(iv) orange rope flagging (or pink/black tape) demarcates Aboriginal heritage areas; and
(v) green flagging around nominated plants for reuse of vegetation.
During site work under the Contract
(c) The Contractor must inspect and maintain the pegging and flagging installed in accordance with Drawing 201928-0001-1.
(d) The Contractor must ensure that the pegging and flagging is clearly visible to all Workers and Short Term Workers for the duration of the work under the Contract.
Post site work 
(e) The Contractor must remove pegging and flagging within 14 days of the Date of Practical Completion.
204B.24.2 Contract Specific Management Requirements
	PEGGING AND FLAGGING
	HOLD / WITNESS POINT

	Nil.
(OR delete this row and amend requirements below as applicable, change text to black)
	

	(a) Insert text of specific flagging and pegging requirements.
	



204B.25	PROPERTY CONDITION
204B.25.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must offer to undertake property condition surveys of all properties and structures that may be affected by the work under the Contract.  As a minimum, the extent of the property condition survey must include:
(i) all properties within 100 metres of any work under the Contract;
(ii) any nearby properties of historical heritage significance which may be impacted by the work under the Contract; and
(iii) any nearby structures of historical heritage significance which may be impacted by the work under the Contract.
(b) The Contractor must ensure that permission and/or agreement from the owner/s and/or occupier/s is given prior to any property condition inspections being undertaken using the Property Condition Survey Notification Letter Template available at Environmental & Heritage Management | Main Roads Western Australia.
(c) Property condition surveys must establish the condition of all properties and structures that may be affected directly or indirectly by the activity.  An individual report (including photographs) must be prepared for each inspected property.
(d) The Contractor must inform relevant owner/occupants of all properties within 100 metres of any construction activities about the nature and timing of the work under the Contract and the contact details for managing complaints.
(e) The Contractor will ensure a procedure is in place for recording all complaints regarding public nuisance, vibration, dust, noise, water damage or property damage.
During site work under the Contract
(f) The Contractor must have procedures for dealing with complaints regarding public nuisance, vibration, dust, noise, water damage or structural damage.  These procedures must ensure that the Superintendent is informed within 24 hours of any such complaint/report.
(g) The Contractor must respond to any complaint or claim of alleged indirect or direct property damage arising from the work under the Contract at the earliest opportunity but no later than 24 hours after the complaint/report.
(h) The Contractor must undertake subsequent investigations resulting from complaints of damage.
Post site work 
(i) The Contractor must undertake property condition surveys of all properties and structures that may be affected by construction at the conclusion of construction.
(j) A copy of the report must be provided to the Superintendent.
204B.25.2 Contract Specific Management Requirements
	PROPERTY CONDITION
	HOLD / WITNESS POINT

	Nil.
(OR delete this row and amend requirements below as applicable, change text to black)
	

	(a) Insert text from Property Survey Condition Report or any other specific stakeholder commitments.
	



204B.26	REVEGETATION / REHABILITATION / LANDSCAPING
204B.26.1 Standard Management Requirements
Refer to Specification 304.
Pre site work under the Contract
(a) Prior to undertaking revegetation, rehabilitation or landscaping all vehicles, machinery, equipment and plant must be checked using the Main Roads Hygiene Checklist (available at https://www.mainroads.wa.gov.au/technical-commercial/contracting-to-main-roads/environmental-heritage-management/) to ensure that they are free of weed bearing material (soil and vegetation), particularly on the treads, tyres, mud flaps and underbody.  Completed checklists are to be retained and provided in the Contractor Reporting specified by the Contract.
During the work under the Contract
(b) While undertaking revegetation, rehabilitation or landscaping, the Contractor must minimise the risk of the introduction and spread of weeds.
(c) The Contractor must ensure that no known weed-affected soil, mulch fill or other material is bought into the area.
Post site work 
Nil.
204B.26.2 Contract Specific Management Requirements
	REVEGETATION / REHABILITATION / LANDSCAPING
	HOLD / WITNESS POINT

	Nil.
(OR delete this row and amend requirements below as applicable, change text to black)
	

	(a) Insert specific Revegetation Management Plan or approvals regarding revegetation requirement.
	



204B.27	SIDETRACKS / TEMPORARY ACCESS TRACKS
Environmental and heritage management requirements for side tracks and temporary access tracks are discussed in other parts of this specification and Specification 202 TRAFFIC MANAGEMENT.
204B.27.2 Contract Specific Management Requirements
	SIDETRACKS / TEMPORARY ACCESS TRACKS
	HOLD / WITNESS POINT

	Nil.
(OR delete this row and amend requirements below as applicable, change text to black)
	

	(a) Insert project-specific requirements for side tracks or temporary access tracks.
	



204B.28	SPECIAL ENVIRONMENTAL AREAS
204B.28.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must peg Special Environmental Areas (SEAs) with orange flagging tape in accordance with Drawing 201928-0001-1 Construction Peg Colour Code (available at https://www.mainroads.wa.gov.au/technical-commercial/technical-library/). 
(b) The pegging of SEAs prior to commencement of site work under the Contract must be approved by the Superintendent. Evidence of Superintendent approval of the SEAs is a HOLD POINT.
(c) The Contractor must ensure that the risk of causing adverse Environmental and Heritage Impacts to SEAs listed in Clause 204B.28.3 Special Environmental Area Locations is avoided.
(d) The Contractor must ensure the flagged area adequately protects the SEA for the duration of the site work under the Contract and includes an appropriate (e.g. 10 metre) buffer, as approved by the Superintendent.  
(e) Where SEAs are within the Limits of Activity, these areas shall be indicated on the Contractor’s site layout figure to be submitted as part of the EMP.
During site work under the Contract
(f) The Contractor must not enter SEA flagged areas, unless permitted by the Superintendent. If access is required, the Contractor must obtain prior written approval from the Superintendent prior to entering the flagged SEA for any reason.
(g) The Contractor must regularly inspect the SEA and the flagging to ensure the SEA is adequately protected from the work under the Contract.
(h) The Contractor must ensure SEAs are not used for storage of materials or equipment.
(i) The Contractor must ensure there is no direct or indirect impact upon SEAs.
(j) If there is disturbance or impact to the SEA, the Contractor must report it as an Environmental Incident within 24 hours of becoming aware of it.
(k) If a SEA is identified during the work under the Contract (other than those listed in Clause 204B.28.3 Special Environmental Area Locations), the Contractor must:
(i) immediately cease all work within 10 metres of the SEA;
(ii) immediately notify the Superintendent;
(iii) protect the area from any (further) disturbance;
(iv) demarcate the area in accordance with SEA pegging and flagging requirements in Clause 204B.24;
(v) implement Operational Controls to prevent impact to the area from any further work under the Contract; and
(vi) not recommence site work under the Contract adjacent to the demarcated area until written approval to proceed is received from the Superintendent.  This is a HOLD POINT.
Post site work 
(l) The Contractor must remove flagging/demarcation around the SEA and any damage to the SEA remediated at the conclusion of the work under the Contract to the satisfaction of the Superintendent.
204B.28.2 Contract Specific Management Requirements
	SPECIAL ENVIRONMENTAL AREAS
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) If a SEA needs to be accessed during the work under the Contract, the following measures must be implemented:
i) Obtain written permission from the Superintendent prior to entering the area.
	

	(b) Insert project specific requirements from environmental and heritage approvals.
	


204B.28.3 Special Environmental Area Locations
	LOCATION
	REFERENCE

	(e.g. Drawing Number, Shapefile, Clearing Map)
DELETE THIS ROW
	i.e. specific elements from the design that need to be detailed.

	
	



204B.29	SPILL AND LEAK MANAGEMENT
204B.29.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must ensure that Operational Controls for spills/leaks are in place prior to the commencement of site work under the Contract.
(b) The Contractor must ensure that appropriate personnel have been trained and are able to implement spill response and containment measures, prior to the commencement of site work under the Contract.
During site work under the Contract
(c) The Contractor must ensure that the risk of spills/leaks causing adverse Environmental and Heritage Impacts are avoided and/or minimised.
(d) The Contractor must ensure that Operational Controls for spills/leak management includes appropriate spill response, containment measures and disposal of contaminated material.
(e) The Contractor must ensure that the spill response and containment measures are readily available to ensure timely response to spills/leaks.
(f) The Contractor must ensure that the spill response and containment measures are appropriate to the volume and type of materials that are at risk of spillage.
(g) The Contractor must regularly inspect and maintain spill response equipment and containment measures to ensure they are fit for purpose.
(h) In the event of a spill/leak, the Contractor must undertake all reasonable actions necessary to minimise Environmental and Heritage Impacts and prevent further Environmental and Heritage Impacts.
(i) The Contractor must contact the Department of Water and Environmental Regulation (DWER) Pollution Response Unit for advice and/or assistance on the management of spills/leaks that may cause significant pollution or environmental harm (Duty to notify of waste discharge, WA (wa.gov.au)).
(j) Spills/leaks must be reported and investigated as an Environmental Incident by the Contractor.
(k) In the event of a spill where the spill cannot be cleaned up immediately, the Contractor must ensure that the cause of the spill has ceased and the spill is appropriately isolated and contained to prevent further adverse Environmental and Heritage Impacts.
(l) The Contractor must clean up to the satisfaction of the Superintendent and dispose of contaminated soil, material and damaged equipment to a location approved by the Superintendent.
Post site work 
(m) At the completion of site work under the Contract, if not already done so, the Contractor must clean up and dispose of any spills/leaks or areas of soil/gravel contamination caused by spill/leaks, to an approved location, to the approval of the Superintendent.
204B.29.2 Contract Specific Management Requirements
	SPILL AND LEAK MANAGEMENT
	HOLD / WITNESS POINT

	Nil.
(OR delete this row and amend requirements below as applicable, change text to black)
	

	(a) Insert specific requirements for spill/leak management.
	



204B.30	STOCKPILE MANAGEMENT
204B.30.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must nominate locations for stockpiling of gravel, concrete, cement, aggregate, rock, overburden, spoil, plant, culverts, dangerous goods, mulch, vegetation and topsoil, and any other materials that require stockpiling, for approval by the Superintendent.
(b) The Contractor must ensure that stockpiles are located:
(i) within the Limits of Activity;
(ii) not within areas of native vegetation;
(iii) not within areas of known or suspected dieback infestation;
(iv) not within areas of known weed infestation;
(v) not within areas identified as Special Environmental Areas (SEAs);
(vi) more than 50 metres from a watercourse, wetland, surface water drainage channel, public drinking water source area or wellhead protection management zone; and
(vii) not within low lying areas subject to inundation or in a way that would impede or restrict drainage or natural surface water flow.
During site work under the Contract
(c) The Contractor must ensure:
(i) ‘suitable’ stockpiles as defined by 204B.22 MULCH AND TOPSOIL are kept free from weeds, dieback and other pathogens;
(ii) stockpile height is no more than 5 metres;
(iii) stockpiles are not affected by erosion or destabilisation; and
(iv) records are maintained for all types of materials stored and stockpiled for use in the Project.
(d) The Contractor must ensure there is sufficient space (e.g. 2 metre wide corridor around all sides) for the storage of stockpiled material and access to the stockpiles in accordance with Drawing 201928-0002 – Stockpile Cross Sections (available at https://www.mainroads.wa.gov.au/technical-commercial/technical-library/).
(e) The Contractor must protect and stabilise stockpiles to minimise erosion, sedimentation and the loss of materials from the stockpile.
(f) Stockpiles are to be segregated and signposted in accordance with Drawing 201928-0002.
Post site work 
(g) All stockpiles are to be removed at the conclusion of site work under the Contract and the area reinstated and rehabilitated to the satisfaction of the Superintendent.
(h) Spoil material will be disposed of at nominated sites approved by the Superintendent.
204B.30.2 Contract Specific Management Requirements
	STOCKPILE MANAGEMENT
	HOLD / WITNESS POINT

	Nil.
(OR delete this row and amend requirements below as applicable, change text to black)
	

	(a) Insert text specific for stockpile management.
	



204B.31	WASTE MANAGEMENT
204B.31.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must implement Operational Controls to ensure that the risk of waste causing adverse Environmental and Heritage Impacts to vegetation, fauna, soil, waterways, groundwater, Aboriginal cultural heritage areas, SEAs or infrastructure is avoided and/or minimised.
(b) The Contractor must identify all the waste streams that may result from the work under the Contract (including demolition waste, contaminated soil), and proposed disposal locations, prior to commencement of site work under the Contract.
(c) The Contractor must ensure all waste disposal locations and recycling facilities meet the requirements of WA State regulations, local government and/or Aboriginal community requirements, prior to commencement of site work under the Contract.  The Superintendent will also approve the proposed waste disposal locations and recycling facilities.
(d) The Superintendent may identify materials on the Site as waste, to be recognised as such by the Contractor, in accordance with the definitions under the Landfill Waste Classification and Waste Definitions 1996.
During site work under the Contract
(e) The Contractor must apply the sustainability hierarchy principals for waste management of avoid, reduce, reuse and recycle.
(f) The Contractor must only dispose of waste at the locations previously approved by the Superintendent.
(g) The Contractor must ensure that waste susceptible of being wind-blown or attracting feral animals, is covered, contained and disposed of regularly at an approved location.
(h) Where local existing waste collection services are not available for the waste streams, the Contractor must organise collection and disposal to an appropriate disposal facility.  Receipts/records of disposal shall be retained as evidence of appropriate disposal.
(i) The Contractor must not bury or burn any waste and not discharge any type of waste to the ground or waterway.
(j) The Contractor must report all waste materials (construction waste, demolition waste and site office waste) disposed at a landfill facility to the Superintendent and via the Contractor Reporting specified by the Contract.
(k) If the Contractor supplies material to a landowner, the Contractor must obtain prior approval from the Superintendent and landowner’s written non-liability consent for receiving the material.  The Contractor must maintain records of the quantities delivered to each location, for reporting to the Superintendent.
Post site work 
(l) The Contractor must ensure that all waste materials (including liquids, excess soil, cement, rubbish, construction waste and debris, and any other deleterious matter) and damaged/unusable equipment is removed and disposed of from the Site at a suitable waste disposal facility.
(m) The Contractor must report final waste and recycling volumes disposed at landfill or recycling facilities, to the Superintendent.
204B.31.2 Contract Specific Management Requirements
	WASTE MANAGEMENT
	HOLD / WITNESS POINT

	Nil.
(OR delete this row and amend requirements below as applicable, change text to black)
	

	(a) Insert text from approvals regarding waste management requirements.
	



204B.32	WATER ABSTRACTION AND STORAGE
204B.32.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must ensure that the risk of water abstraction and storage causing adverse Environmental and Heritage Impacts is avoided and/or minimised.
(b) If the water is Contractor supplied, the Contractor must obtain the necessary licence and approvals for the taking of and accessing water from the proposed locations, prior to commencing site work under the Contract, in accordance with the relevant legislation.
(c) The Contractor must ensure the water quality, for example being free from high salt content and dieback, is suitable for its intended use under the Contract.
(d) If the water is Principal supplied, the Contractor must comply with Specification 303 MATERIAL AND WATER SOURCES for the access and use of any water source.
(e) All water sources to be used are to be approved by the Superintendent prior to water abstraction commencing.  Superintendent approval of water sources is a HOLD POINT (in accordance with Specification 303 MATERIALS AND WATER SOURCES).
(f) The Contractor must install temporary fencing and/or signage around water storage locations to prevent water being used for inappropriate activities.
During site work under the Contract
(g) The Contractor must prevent water from being wasted and ensure it is reused wherever practicable.
(h) The Contractor must ensure that livestock have unhindered access to pre-existing water points or station water supplies during the course of the work under the Contract.
(i) The Contractor must maintain records and populate the water usage details in the Contractor Reporting specified by the Contract.
(j) For Principal nominated water sources, the Contractor must reference the IRIS reference number as stated in Table 303D.1 when populating the water usage details in the Contractor Reporting specified by the Contract.
Post site work 
(k) The Contractor is responsible for leaving the water abstraction location in a safe and stable condition at the conclusion of the work under the Contract, to the satisfaction of the Superintendent.
(l) The Contractor is responsible for communicating any ongoing water management or handover of bore/infrastructure requirements (if required) to the Superintendent at the conclusion of the work under the Contract.
204B.32.2 Contract Specific Management Requirements
	WATER ABSTRACTION AND STORAGE
	HOLD / WITNESS POINT

	Nil.
(OR delete this row and amend requirements below as applicable, change text to black)
	

	(a) Insert text from project specific water licence requirements or Bed and Banks approval.
	



204B.33	WATER DRAINAGE MANAGEMENT
204B.33.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must ensure that site work under the Contract does not cause adverse Environmental and Heritage Impacts, obstruct, or contaminate any water courses or drainage ways.
During site work under the Contract
(b) The Contractor must undertake the work under the Contract with minimal disturbance to riparian vegetation and bed and banks of a watercourse.
(c) The Contractor must ensure that the work under the Contract does not cause harm, contaminate or structurally change a watercourse or wetland.
(d) The Contractor must ensure storm events are monitored and the potential Environmental and Heritage Impacts of contaminated stormwater runoff from the Site into the environment is minimised.
(e) The Contractor must avoid generating contaminated stormwater by diverting stormwater away from areas of exposed contaminated soil.
(f) The Contractor must ensure that existing natural or artificial drainage lines within the Site are maintained and water flows are not blocked or adversely obstructed/restricted.
(g) The Contractor must ensure that the work under the Contract does not act as an artificial barrier or levee in waterways and drainage systems.
(h) The Contractor is not to discharge water offsite without prior approval from the Superintendent.
(i) The Contractor must ensure that all surfaces are shaped to avoid pooling or ponding.
(j) The Contractor must report an Environmental Incident if the quality and/or flow of water is adversely impacted by the work under the Contract.
(k) The Contractor must always maintain waterways and drainage systems in proper working order for the duration of the work under the Contract.
Post site work 
(l) The Contractor must stabilise disturbed areas to the approval of the Superintendent following the completion of site work under the Contract to ensure no adverse effects to water resources.
(m) The Contractor must dispose of all water stored during the work under the Contract, to the satisfaction of the Superintendent.
(n) The Contractor must ensure culvert and drainage structures are free of blockages including, but not limited to, vegetation, soil, waste and debris.
204B.33.2 Contract Specific Management Requirements
	WATER DRAINAGE MANAGEMENT
	HOLD / WITNESS POINT

	Nil.
(OR delete this row and amend requirements below as applicable, change text to black)
	

	(a) Insert text from approvals regarding water management.
	



204B.34	WEED MANAGEMENT
204B.34.1 Standard Management Requirements
Pre site work under the Contract
(a) The Contractor must ensure that the risk of spreading weeds causing adverse Environmental and Heritage Impacts is avoided and/or minimised.
(b) Prior to commencing site work under the Contract, all vehicles, machinery, equipment and plant must be checked using the Main Roads Hygiene Checklist (available at https://www.mainroads.wa.gov.au/technical-commercial/contracting-to-main-roads/environmental-heritage-management/) to ensure that they are free of weed bearing material (soil and vegetation), particularly on the treads, tyres, mud flaps and underbody. Completed checklists are to be retained and provided in the Contractor Reporting specified by the Contract.
(c) The Contractor must have procedures in place if vehicles, machinery and plant arrive on site that do not meet hygiene standards.
During site work under the Contract
(d) The Contractor must monitor the Site for new declared and/or invasive weed species and ensure that these weeds are controlled.
(e) The Contractor must ensure that no known weed, pest or diseased affected soil, mulch, fill or other material is brought to site.
(f) During clearing activities, the Contractor must signpost weed infested stockpiled material in a location approved by the Superintendent.
(g) The Contractor must control any weeds germinating on stockpiles and maintain records of weed spraying using the Main Roads Vegetation Maintenance Record Forms (available at https://www.mainroads.wa.gov.au/technical-commercial/contracting-to-main-roads/environmental-heritage-management/) and submit to the Superintendent within 14 days of the treatment.
(h) The Contractor must treat weed infestations if they arise, as directed by the Superintendent.
(i) The Contractor must provide evidence to the Superintendent that weed control has been conducted (if required).
(j) Any herbicide application shall be carried out by qualified and experienced personnel, in a manner that prevents overspray from reaching waterways, drainage lines or threatened species.
Post site work 
Nil.
204B.34.2 Contract Specific Management Requirements
	WEED MANAGEMENT
	HOLD / WITNESS POINT

	Nil.
(OR delete this row, add contract specific management requirements below as applicable (suggested examples are provided in blue text) and change text to black)
	

	(a) The Contractor must remove or kill any weeds on an annual basis (or at least once during the work under the Contract), that are growing within cleared areas, where those weeds are likely on the advice of the Principal, to spread and result in environmental harm to adjacent areas of native vegetation that are in good or better condition.  The location for the weed control is in Clause 204B.34.3.
	

	(b) The Contractor must remove all weed infested stockpiles, as shown in Clause 204B.34.4 at the conclusion of the site work under the Contract, to the satisfaction of the Superintendent.
	

	(c) If using CPS 818: Prior to leaving the Site, all vehicles, machinery, equipment and plant must be inspected using the Main Roads Hygiene Checklist (available at https://www.mainroads.wa.gov.au/technical-commercial/contracting-to-main-roads/environmental-heritage-management/) to ensure that they are free of soil and vegetation, particularly on tread, tyres, mud flaps and underbody.  Completed checklists are to be retained and provided in the Contractor Reporting specified by the Contract.
	

	(d) The Contractor must provide copies of the completed herbicide spray register, records of weed control activities and Hygiene Checklists for both entry and exit of vehicles and machinery, within fourteen (14) business days of Date of Practical Completion.
	

	(e) Insert text from requirements to manage Declared Pests/Weeds that may spread and harm adjacent native vegetation in good or better condition or specific weeds in nominated locations.
	


204B.34.3 Nominated Weed Management Locations
	LOCATION
	REFERENCE

	(e.g. Drawing Number, Shapefile, Clearing Map)
DELETE THIS ROW
	

	
	


204B.34.4 Nominated Weed Infested Spoil / Topsoil / Mulch For Removal Locations
	LOCATION
	REFERENCE

	(e.g. Drawing Number, Shapefile, Clearing Map)
DELETE THIS ROW
	

	
	



204B.35	OTHER PROJECT MANAGEMENT REQUIREMENTS
204B.35.1 Standard Management Requirements
Nil.
204B.35.2 Contract Specific Management Requirements
	OTHER PROJECT MANAGEMENT REQUIREMENTS
	HOLD / WITNESS POINT

	Nil.
(OR delete this row and amend requirements below as applicable, change text to black)
	

	(a) Requirements for road marking, vibration, sealing, priming, sweeping, spoil management and traffic management need to be considered here.
	

	(b) Insert text from project specific requirements
	





GUIDANCE NOTES
FOR REFERENCE ONLY – DELETE GUIDANCE NOTES FROM FINAL DOCUMENT

1. All edits to this specification are to be made using track changes, to clearly show added/ deleted text.
More information about environmental management in Construct Only Contracts is available in D21#131721.
If all information relating to a clause is deleted, the clause number should be retained and the words “NOT USED” should be inserted.
The proposed document with tracked changes must be submitted to the Project Manager for review, prior to finalising the document.
Once the Project Manager’s review is complete, accept all changes in the document, turn off track changes and refresh the Table of Contents.
The Custodian of this specification is Director Environment and Heritage.
	
Note: Specification 204 is applicable to all contracts. 
Specification 204 requires the Contractor to develop and implement an EMP.  Where a PEWR is provided by the Principal, the Contractor is not required to develop an EMP, but instead must comply with, and sign-on to, the controls listed in the PEWR.
This specification lays out the Principal’s minimum environmental and heritage requirements that the Contractor must develop and detail in the EMP to deliver the work under the Contract.  The EMP template will assist the Contractor in developing an EMP.
INSTRUCTIONS FOR COMPLETING THE ANNEXURES
1. Prior to populating Specification 204B for construction works, it is recommended that the Project Development and Deliver Environmental and Heritage Logistics Considerations Checklist (D19#469684) is referred to and discussed with the relevant Environmental Officer (EO).
2. Determine which document the Contractor will utilise for the work under the Contract (see Table 1 for selection choices) and delete the other two documents from Annexure 204A:
(a) Construction Environmental Management Plan (CEMP) 
(b) Maintenance Environmental Management Plan (MEMP) 
(c) Principal Environmental Works Requirements (PEWR) 

Table 1: Environmental Management Plan Selection
	EMP Option
	Resources
	When to choose

	CEMP
(Template at D23#605864)
	Environmental Assessment, Approvals and Compliance Process iRoads Page
Environmental Management in Construct Only Contracts Procedure (D21#131721)

	Construction project with: 
· Moderate environmental complexities 
· Major environmental complexities with environmental approvals
· Greater environmental risks
· Longer timeframe, months rather than weeks
· Scale of works, several hectares or kilometres.

	MEMP
(Template at D25#669741)

	Maintenance Environmental Management iRoads Page
Maintenance Environmental Management Procedure 
(D17#694712)
	Maintenance works with:
· Major environmental complexities with environmental approvals
· Many different maintenance tasks
· Longer timeframe, months rather than weeks
· Scale of works, several hectares or several roads
· Grid Replacements, Bridge, Culvert, Drainage Works, Road Surface, Shoulder, Pavement Rehabilitation.

	PEWR
(Template at D22#1094510)

	Environmental Assessment, Approvals and Compliance Process iRoads Page
Maintenance Environmental Management iRoads Page
	Construction or maintenance works with:
· Low environmental risks, less complex works
· Shorter timeframes
· Smaller scale
· Pavement Repair, Sweeping, Sumps, Grids, Signs, Roadside Litter Collection, Floodways, Parking Bays & Rest Areas, Dangerous Trees, Traffic Management.



3. If a standard management clause in Annexure 204B is not relevant to the work under the Contract, it will be deleted by the EO and replaced with ‘NOT USED’ (the clause number is to be retained).
4. The EO will populate the tables for Contract Specific Management Requirements in Annexure 204B with the compliance requirements from the regulatory approvals that are to be assigned to the Contractor, if applicable (suggested examples are provided in blue text).
5. The EO will determine whether a HOLD POINT or WITNESS POINT is required for any Contract Specific Management Requirement, and enter them into the table accordingly.
6. The EO is to populate and align the standard and contract specific management requirements in Specification Annexure 204B with the standard management requirements in the chosen EMP document.  Clauses that are not relevant to the work under the Contract will be deleted and replaced with ‘NOT USED’ in the EMP.
7. The partially populated EMP template will be supplied in Specification Annexure 204A to the Contractor for completion.
8. The Contractor is not required to populate a PEWR or submit for a suitability check if provided in Annexure 204A.  However, the PEWR is to be signed by all on site contractors and subcontractors.
9. If a Principal-nominated aggregate laydown is proposed to be used, the EO needs to access the Aggregate Laydown Register (D23#173360) to determine the site specific management requirements to be entered into Clause 204B 20.2.
10. Clause 204B 35.2 Other Project Management Requirements will be used to refer to requirements for road marking, vibration, sealing, priming, sweeping, spoil management and traffic management that have been removed from this version of Specification 204, as well as any other requirement that does not fit into the pre-defined clauses.
11. Please refer to the latest environmental procedures and information available at Construct Only Contracts on iRoads.



CONTRACT SPECIFIC REQUIREMENTS
The following clauses are to be placed under the CONTRACT SPECIFIC REQUIREMENTS, as required.  After inserting the clause, change the clause number and heading to style “H2 SP” so it appears in the Table of Contents.

	XXX.XX	SUB-HEADING (H2 SP)
	

	1. Insert text (Main Table SP)
	XXXX

	Insert text (Main Table SP)
	

	XXX.XX	SUB-HEADING (H2 SP)
	

	1. Insert text (Main Table SP)
	

	Insert text (Main Table SP)
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