ORD MRWA Barrier line - README

Updated process removes the need for the *ORD to MX Transformation Spreadsheet - Blank*

# Configuration

Copy:

MRWA-Overtaking\_Sight\_Visibility\_Report-DesignSpeed.xsl

To:

C:\ProgramData\Bentley\OpenRoads Designer CE\Configuration\Organization-Civil\ANZ Design\Reports\Evaluation ANZ

# Process

1. Run OpenRoads Sight Visibility
2. Create report using *MRWA-Overtaking\_Sight\_Visibility\_Report-DesignSpeed.xsl*
3. Copy report data and past into *ORD Barrier-Line-Spreadsheet Blank .xlsm*

## Refer to video

ORD- MRWA\_barrier\_line\_spreadsheet\_EXAMPLE.mp4